{"text_format":"3","workbook":"xls","n_sheets":7,"sheets":["Macro1","评标各分部分析表","封面","报价汇总","21F装修","12F机电安装","总价措施费项目"],"not_rendered":{"images":1,"external_links":1,"defined_names":7},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":7,"n_cols":1,"rows_kept":7,"hidden":true,"flags":["formulas_cached_only"]}
[]
[true]
[{"$error":"#N/A"}]
[{"$error":"#N/A"}]
[{"$error":"#N/A"}]
[false]
[true]

{"sheet":"评标各分部分析表","index":1,"n_rows":76,"n_cols":7,"rows_kept":76,"hidden":true,"merged":[[0,0,0,6],[73,2,73,4]],"flags":["formulas_cached_only"]}
["园林工程标底费用分析表"]
["序号","分部分项名称","人工费（元）","主材费（元）","其他费用（元）","合计(元)","各分部占总造价比列"]
[null,"园林建筑工程部分",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[1,"LD-1.04标准车道种植槽道牙详图(柏油路)",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[2,"LD-1.04标准车道/种植槽道牙详图(人行道)",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[3,"LD-1.05标准树环详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[4,"LD-1.06标准种植槽墙详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[5,"LD-1.07至1.07.1标准种植槽墙座墙详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[6,"LD-1.08标准排水沟详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[7,"LD-1.09标准阶梯式种植槽详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[8,"LD-1.10标准阶梯式草坪详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[9,"LD-1.11标准挡土墙详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十","LD-2.01标准台阶详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十一","LD-2.02标准座墙详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十二","LD-2.06至2.06.2标准私家围墙详图",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十三",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十四",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十五",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十六",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十七",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十八",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["十九",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[20,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[21,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[22,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[23,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[24,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[25,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[26,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[27,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[28,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[29,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[30,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[31,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[32,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[33,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[34,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[35,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[36,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[37,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[38,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[39,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[40,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[41,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[42,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[43,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[44,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[45,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[46,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[47,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[48,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[49,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[50,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[51,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[52,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[53,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[54,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[55,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[56,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[57,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[58,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[59,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[60,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[61,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[62,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[63,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,"园林水电工程部分",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["一",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["二",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["三",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,"园林绿化工程部分",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["一","栽植乔灌木",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["二","栽植地被",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,"开办费部分",{"$nulls":3},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,"园林工程汇总",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,"各项费用所占总造价比例",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]

{"sheet":"封面","index":2,"n_rows":29,"n_cols":1,"rows_kept":29,"merged":[[0,0,0,8],[14,0,14,8],[15,0,15,8],[19,0,19,8],[29,0,29,8],[30,0,30,8]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[" "]
[" "]
[" "]
[]
[]
[]
[" "]
[" "]
[" "]
[" "]
["横琴南光大厦项目１２F"]
["北大荒办公室精装修工程"]
[" "]
[" "]
[" "]
["工 程 量 清 单 报 价 表"]
[" "]
[" "]
[" "]
[" "]
[" "]
[" "]
[" "]
[" "]
[" "]

{"sheet":"报价汇总","index":3,"n_rows":10,"n_cols":6,"rows_kept":10,"merged":[[0,0,0,5],[7,2,7,4],[8,3,8,5],[9,4,9,5]],"flags":["formulas_cached_only"]}
["横琴南光大厦项目精装修工程报价汇总表"]
["工程名称：横琴南光大厦项目12F北大荒办公室精装修工程"]
["序号","名称","金额(元)","面积\n(m²)","单方造价\n(元/m²)","备注"]
["一","12Ｆ装修工程",null,{"v":617,"d":"617.00"},{"v":0,"d":"0.00"}]
["二","12Ｆ机电工程",null,{"v":617,"d":"617.00"},{"v":0,"d":"0.00"}]
["三","措施项目费",null,{"v":617,"d":"617.00"},{"v":0,"d":"0.00"}]
["四","总造价（含增值税9%）",{"v":0,"d":"0.00"},{"v":617,"d":"617.00"},{"v":0,"d":"0.00"}]
[null,"大写（人民币）",0]
[]
[{"$nulls":4},"日期：   年   月   日"]

{"sheet":"21F装修","index":4,"n_rows":193,"n_cols":14,"rows_kept":193,"merged":[[0,1,0,13],[1,1,1,8],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,2,12],[2,13,3,13],[4,2,4,3],[10,2,10,3],[19,2,19,3],[55,2,55,3],[76,2,76,3],[99,2,99,3],[118,2,118,3],[135,2,135,3],[152,2,152,3],[164,2,164,3],[192,2,192,3]],"flags":["formulas_cached_only"]}
[null,"横琴南光大厦项目工程报价清单（装修）"]
[null,"工程名称：横琴南光大厦项目12F北大荒办公室精装修工程"]
[null,"序号","项目名称","项目特征描述","计量单位","工程量","含税综合单价（元）","其中(元)",{"$nulls":5},"含税合价（元）\n"]
[{"$nulls":7},"人工","主材（含损耗）","机械费及辅材费等","管理费","利润","税金9%"]
[1,"一","拆除基础工程"]
[null,1,"原墙体拆除","人工拆除／打包搬运下楼／车辆清运","m2",{"v":123.10199999999999,"d":"123.10"}]
[null,2,"原吊顶拆除","人工拆除／打包搬运下楼／车辆清运","m2",{"v":570,"d":"570.00"}]
[null,3,"原玻璃门拆除","人工拆除／打包搬运下楼／车辆清运","樘",{"v":3,"d":"3.00"}]
[null,4,"原电路及设备拆除","人工拆除／打包搬运下楼／车辆清运","项",{"v":1,"d":"1.00"}]
[null,5,"原地脚线拆除","人工拆除／打包搬运下楼／车辆清运","项",{"v":1,"d":"1.00"}]
[1,"二","新建基础工程"]
[null,1,"原墙体拆除后墙地面基础修补","陶粒／水泥砂／人工辅料","米",{"v":59.309999999999995,"d":"59.31"}]
[null,2,"原墙体拆除后墙地面饰面修补","墙布／硬包／不锈钢等人工辅料","项",{"v":1,"d":"1.00"}]
[null,3,"原预留卫生间位地面回填","陶粒／水泥砂／人工辅料","m2",{"v":10.8,"d":"10.80"}]
[null,4,"轻钢龙骨隔墙（吊顶以下部分）","75系列轻钢龙骨@400,12mm阻燃胶合板+12mm纸面石膏板间墙基层完成面(间墙内空腔填充吸音棉)\n","m2",{"v":179.2,"d":"179.20"}]
[null,5,"轻钢龙骨隔墙（吊顶以下部分）","150系列轻钢龙骨@400,12mm阻燃胶合板+12mm纸面石膏板间墙基层完成面(间墙内空腔填充吸音棉)\n","m2",{"v":14.559999999999999,"d":"14.56"}]
[null,6,"轻钢龙骨隔墙（吊顶以上部分）","75系列轻钢龙骨@400,12mm阻燃胶合板+12mm纸面石膏板间墙基层完成面(不减管道／梁位／风管等计算)\n","m2",{"v":84,"d":"84.00"}]
[null,7,"轻质砖隔墙（吊顶以下部分）","200轻质砖／水泥砂／人工辅料","m2",{"v":22.4,"d":"22.40"}]
[null,8,"轻质砖隔墙（吊顶以上部分）","200轻质砖／水泥砂／人工辅料(不减管道／梁位／风管等计算)\n","m2",{"v":9.6,"d":"9.60"}]
[1,"三","前台／休闲区/茶水间／开放式办公区"]
[null,"Ａ","天花"]
[null,1,"石膏板吊平顶","50系列轻钢龙骨，双层12mm厚石膏板（投影展开计算）\n","m2",{"v":175,"d":"175.00"}]
[null,2,"石膏板吊顶造型收口边","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":55,"d":"55.00"}]
[null,3,"石膏板吊顶窗帘盒","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":50,"d":"50.00"}]
[null,4,"石膏板灯槽吊顶","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","m2",{"v":17,"d":"17.00"}]
[null,5,"吊顶刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":190,"d":"190.00"}]
[null,6,"石膏板吊顶风口制作","人工辅料","个",{"v":3,"d":"3.00"}]
[null,6,"石膏板吊顶灯具开圆孔","人工辅料","个",{"v":42,"d":"42.00"}]
[null,7,"吊顶定制不锈钢造型线条","定制不锈钢造型线条／人工辅料","米",{"v":30.6,"d":"30.60"}]
[null,8,"木纹铝条格栅吊顶原楼板喷深色涂料处理","深色乳胶漆／人工辅料","m2",{"v":200,"d":"200.00"}]
[null,9,"木纹铝条格栅吊顶","50*100木纹铝条格栅隔150铺装／人工辅料","m2",{"v":190,"d":"190.00"}]
[null,"Ｂ","地面"]
[null,1,"地面水泥砂找平处理","水泥砂／人工辅料","项",{"v":1,"d":"1.00"}]
[null,2,"CP-01方块地毯","CP-01方块地毯，专用胶泥（硬底胶贴）\n","m2",{"v":256,"d":"256.00"}]
[null,3,"ST-01岩板","1220*2440岩板／瓷砖胶粘贴／人工辅料","m2",{"v":110,"d":"110.00"}]
[null,4,"3mm不锈钢线条","3mm不锈钢线条/玻璃胶／人工辅料\n","m",{"v":20,"d":"20.00"}]
[null,"Ｃ","墙面"]
[null,1,"前台背景造型基底制作","12mm阻燃胶合板／人工辅料","m2",20.52]
[null,2,"前台背景造型制作","木饰面／不锈钢／灯片／人工辅料","m2",20.52]
[null,3,"前台公司LOGO字制作及安装","不锈钢字／亚克力发光字等人工辅料","项",{"v":1,"d":"1.00"}]
[null,4,"前台制作","木饰面／大理石／人工辅料","米",{"v":5.5,"d":"5.50"}]
[null,5,"企业文化展示墙背景造型基底制作","12mm阻燃胶合板／人工辅料","m2",{"v":23.004,"d":"23.00"}]
[null,6,"企业文化展示墙背景造型制作","木饰面／不锈钢／灯片／人工辅料","m2",{"v":23,"d":"23.00"}]
[null,7,"企业文化展示墙公司LOGO字制作及安装","不锈钢字／亚克力发光字等人工辅料","项",{"v":1,"d":"1.00"}]
[null,8,"企业文化展示位固定椅制作","12mm阻燃胶合板／木饰面／人工辅料","米",{"v":4.7,"d":"4.70"}]
[null,9,"门套基底制作","12mm阻燃胶合板／人工辅料","米",{"v":11.4,"d":"11.40"}]
[null,10,"安装不锈钢门套","不锈钢／人工辅料","米",{"v":11.4,"d":"11.40"}]
[null,11,"玻璃门预埋基架制作","５０Ｌ镀锌角铁／人工辅料","米",{"v":6,"d":"6.00"}]
[null,12,"玻璃门","12mm电雾化超白玻璃／含设备","m2",14.28]
[null,13,"玻璃门（电机）","电机","套",{"v":1,"d":"1.00"}]
[null,14,"玻璃门锁具五金配件","门夹／地弹／锁具人工辅料","套",{"v":1,"d":"1.00"}]
[null,15,"玻璃门定制拉手","定制不锈钢拉手／人工辅料","副",{"v":1,"d":"1.00"}]
[null,16,"不锈钢脚线基底制作","9mm阻燃胶合板／人工辅料","米",{"v":85,"d":"85.00"}]
[null,17,"安装造型不锈钢脚线","不锈钢／人工辅料","米",{"v":85,"d":"85.00"}]
[null,18,"墙面刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":202.5,"d":"202.50"}]
[1,"四","会议室"]
[null,"Ａ","天花"]
[null,1,"石膏板造型吊顶","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":16.2,"d":"16.20"}]
[null,2,"石膏板吊顶窗帘盒","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":8.8,"d":"8.80"}]
[null,3,"吊顶刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":12.7,"d":"12.70"}]
[null,4,"MT-03铝单板吊顶","MT-03铝单板／人工辅料","m2",{"v":30.3,"d":"30.30"}]
[null,5,"MT-03铝单板吊顶灯槽","MT-03铝单板／人工辅料","米",{"v":15.2,"d":"15.20"}]
[null,"Ｂ","地面"]
[null,1,"地面水泥砂找平处理","水泥砂／人工辅料","项",{"v":1,"d":"1.00"}]
[null,2,"CP-02方块地毯","CP-02方块地毯，专用胶泥（硬底胶贴）\n","m2",{"v":39,"d":"39.00"}]
[null,3,"3mm不锈钢线条","3mm不锈钢线条/玻璃胶／人工辅料\n","m",{"v":3.9,"d":"3.90"}]
[null,"Ｃ","墙面"]
[null,1,"墙面木饰面基底制作","9mm阻燃胶合板／人工辅料","m2",19.71]
[null,2,"墙面木饰面","木饰面／人工辅料","m2",19.71]
[null,3,"门套基底制作","12mm阻燃胶合板／人工辅料","米",9.32]
[null,4,"安装不锈钢门套","不锈钢／人工辅料","米",9.32]
[null,5,"玻璃隔断","12mm电雾化超白玻璃／含设备","m2",{"v":10.584,"d":"10.58"}]
[null,6,"玻璃门锁具五金配件","门夹／地弹／锁具人工辅料","套",{"v":1,"d":"1.00"}]
[null,7,"玻璃门定制拉手","定制不锈钢拉手／人工辅料","副",{"v":1,"d":"1.00"}]
[null,8,"不锈钢脚线基底制作","9mm阻燃胶合板／人工辅料","米",{"v":7.3,"d":"7.30"}]
[null,9,"安装造型不锈钢脚线","不锈钢／人工辅料","米",{"v":7.3,"d":"7.30"}]
[1,"五","储物间／洽谈室／机房/打印室"]
[null,"Ａ","天花"]
[null,1,"石膏板吊顶","50系列轻钢龙骨，双层12mm厚石膏板\n","m2",{"v":18,"d":"18.00"}]
[null,2,"石膏板吊顶窗帘盒","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":2.7,"d":"2.70"}]
[null,3,"玻璃隔断位吊顶加固","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",4.86]
[null,4,"石膏板吊顶开排风口","人工辅料","个",{"v":3,"d":"3.00"}]
[null,5,"石膏板吊顶开灯孔","人工辅料","个",{"v":5,"d":"5.00"}]
[null,6,"吊顶刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":19.2,"d":"19.20"}]
[null,"Ｂ","地面"]
[null,1,"地面水泥砂找平处理","水泥砂／人工辅料","项",{"v":1,"d":"1.00"}]
[null,2,"CP-02方块地毯","CP-02方块地毯，专用胶泥（硬底胶贴）\n","m2",{"v":11.6,"d":"11.60"}]
[null,3,"CT-01地砖","600*600地砖／人工辅料\n","m2",{"v":5.2,"d":"5.20"}]
[null,4,"3mm不锈钢线条","3mm不锈钢线条/玻璃胶／人工辅料\n","m",5.86]
[null,"Ｃ","墙面"]
[null,1,"机房隔断及门","木饰面／含五金配件锁具","m2",6.24]
[null,2,"不锈钢门套基底制作","12mm阻燃胶合板／人工辅料","米",{"v":10.2,"d":"10.20"}]
[null,3,"安装不锈钢门套","不锈钢／人工辅料","米",{"v":10.2,"d":"10.20"}]
[null,4,"墙面刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":54.6,"d":"54.60"}]
[null,5,"玻璃隔断","12mm电雾化超白玻璃／含设备","m2",17.16]
[null,6,"玻璃门锁具五金配件","门夹／地弹／锁具人工辅料","套",{"v":1,"d":"1.00"}]
[null,7,"玻璃门定制拉手","定制不锈钢拉手／人工辅料","副",{"v":1,"d":"1.00"}]
[null,8,"不锈钢脚线基底制作","9mm阻燃胶合板／人工辅料","米",{"v":21,"d":"21.00"}]
[null,9,"安装造型不锈钢脚线","不锈钢／人工辅料","米",{"v":21,"d":"21.00"}]
[1,"六","董事长办公室"]
[null,"Ａ","天花"]
[null,1,"石膏板造型吊顶","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","m2",{"v":18.6,"d":"18.60"}]
[null,2,"石膏板吊顶灯槽","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":23.1,"d":"23.10"}]
[null,3,"石膏板吊顶窗帘盒","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":12.2,"d":"12.20"}]
[null,4,"石膏板吊顶开灯孔","人工辅料","个",{"v":15,"d":"15.00"}]
[null,5,"石膏板吊顶风口","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":6.5,"d":"6.50"}]
[null,6,"吊顶刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":21.6,"d":"21.60"}]
[null,"Ｂ","地面"]
[null,1,"铺装门槛石","大理石／人工辅料","米",{"v":1,"d":"1.00"}]
[null,2,"地面水泥砂找平处理","水泥砂／人工辅料","项",{"v":1,"d":"1.00"}]
[null,3,"CP-02方块地毯","CP-02方块地毯，专用胶泥（硬底胶贴）\n","m2",{"v":32.1,"d":"32.10"}]
[null,4,"3mm不锈钢线条","3mm不锈钢线条/玻璃胶／人工辅料\n","m",{"v":1,"d":"1.00"}]
[null,"Ｃ","墙面"]
[null,1,"墙面木饰面基底制作","9mm阻燃胶合板／人工辅料","m2",{"v":16.900000000000002,"d":"16.90"}]
[null,2,"墙面木饰面","木饰面／人工辅料","m2",{"v":16.9,"d":"16.90"}]
[null,3,"墙面刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",35.36]
[null,4,"不锈钢脚线基底制作","9mm阻燃胶合板／人工辅料","米",{"v":12.6,"d":"12.60"}]
[null,5,"安装造型不锈钢脚线","不锈钢／人工辅料","米",{"v":12.6,"d":"12.60"}]
[1,"七","总经理办公室"]
[null,"Ａ","天花"]
[null,1,"石膏板造型吊顶","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","m2",{"v":15.6,"d":"15.60"}]
[null,2,"石膏板吊顶灯槽","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":21.8,"d":"21.80"}]
[null,3,"石膏板吊顶窗帘盒","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",4.97]
[null,4,"石膏板吊顶开灯孔","人工辅料","个",{"v":11,"d":"11.00"}]
[null,5,"石膏板吊顶风口","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":14.3,"d":"14.30"}]
[null,6,"吊顶刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":34.6,"d":"34.60"}]
[null,"Ｂ","地面"]
[null,1,"铺装门槛石","大理石／人工辅料","米",{"v":1,"d":"1.00"}]
[null,2,"地面水泥砂找平处理","水泥砂／人工辅料","项",{"v":1,"d":"1.00"}]
[null,3,"CP-02方块地毯","CP-02方块地毯，专用胶泥（硬底胶贴）\n","m2",{"v":26,"d":"26.00"}]
[null,4,"3mm不锈钢线条","3mm不锈钢线条/玻璃胶／人工辅料\n","m",{"v":1,"d":"1.00"}]
[null,"Ｃ","墙面"]
[null,1,"墙面刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":50.7,"d":"50.70"}]
[null,2,"不锈钢脚线基底制作","9mm阻燃胶合板／人工辅料","米",{"v":19.5,"d":"19.50"}]
[null,3,"安装造型不锈钢脚线","不锈钢／人工辅料","米",{"v":19.5,"d":"19.50"}]
[1,"八","副总经理办公室"]
[null,"Ａ","天花"]
[null,1,"石膏板造型吊顶","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","m2",{"v":12.2,"d":"12.20"}]
[null,2,"石膏板吊顶灯槽","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":22.3,"d":"22.30"}]
[null,3,"石膏板吊顶窗帘盒","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":3.3,"d":"3.30"}]
[null,4,"石膏板吊顶开灯孔","人工辅料","个",{"v":11,"d":"11.00"}]
[null,5,"石膏板吊顶风口","50系列轻钢龙骨，12mm胶合板加12mm厚石膏板\n","米",{"v":10,"d":"10.00"}]
[null,6,"吊顶刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":27.8,"d":"27.80"}]
[null,"Ｂ","地面"]
[null,1,"铺装门槛石","大理石／人工辅料","米",{"v":1,"d":"1.00"}]
[null,2,"地面水泥砂找平处理","水泥砂／人工辅料","项",{"v":1,"d":"1.00"}]
[null,3,"CP-02方块地毯","CP-02方块地毯，专用胶泥（硬底胶贴）\n","m2",{"v":26.5,"d":"26.50"}]
[null,4,"3mm不锈钢线条","3mm不锈钢线条/玻璃胶／人工辅料\n","m",{"v":1,"d":"1.00"}]
[null,"Ｃ","墙面"]
[null,1,"墙面刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":52,"d":"52.00"}]
[null,2,"不锈钢脚线基底制作","9mm阻燃胶合板／人工辅料","米",{"v":19,"d":"19.00"}]
[null,3,"安装造型不锈钢脚线","不锈钢／人工辅料","米",{"v":19,"d":"19.00"}]
[1,"九","财务室"]
[null,"Ａ","天花"]
[null,1,"铝扣板吊顶","铝扣板吊顶／人工辅料","m2",{"v":23.7,"d":"23.70"}]
[null,"Ｂ","地面"]
[null,1,"铺装门槛石","大理石／人工辅料","米",{"v":1,"d":"1.00"}]
[null,2,"地面水泥砂找平处理","水泥砂／人工辅料","项",{"v":1,"d":"1.00"}]
[null,3,"CP-02方块地毯","CP-02方块地毯，专用胶泥（硬底胶贴）\n","m2",{"v":23.7,"d":"23.70"}]
[null,4,"3mm不锈钢线条","3mm不锈钢线条/玻璃胶／人工辅料\n","m",{"v":1,"d":"1.00"}]
[null,"Ｃ","墙面"]
[null,1,"墙面刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":41.6,"d":"41.60"}]
[null,2,"不锈钢脚线基底制作","9mm阻燃胶合板／人工辅料","米",{"v":1,"d":"1.00"}]
[null,3,"安装造型不锈钢脚线","不锈钢／人工辅料","米",{"v":1,"d":"1.00"}]
[1,"十","男／女更衣室"]
[null,"Ａ","天花"]
[null,1,"石膏板吊顶","50系列轻钢龙骨，双层12mm厚石膏板\n","m2",{"v":15,"d":"15.00"}]
[null,2,"石膏板吊顶开排风口","人工辅料","个",{"v":2,"d":"2.00"}]
[null,3,"石膏板吊顶开灯孔","人工辅料","个",{"v":4,"d":"4.00"}]
[null,4,"吊顶刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":15,"d":"15.00"}]
[null,"Ｂ","地面"]
[null,1,"铺装门槛石","大理石／人工辅料","米",{"v":1,"d":"1.00"}]
[null,2,"地面水泥砂找平处理","水泥砂／人工辅料","项",{"v":1,"d":"1.00"}]
[null,3,"CT-01地砖","600*600地砖／人工辅料\n","m2",{"v":15,"d":"15.00"}]
[null,4,"3mm不锈钢线条","3mm不锈钢线条/玻璃胶／人工辅料\n","m",{"v":1,"d":"1.00"}]
[null,"Ｃ","墙面"]
[null,1,"墙面刷PT-01无机涂料","PT-01无机涂料／人工辅料","m2",{"v":62.400000000000006,"d":"62.40"}]
[null,2,"不锈钢脚线基底制作","9mm阻燃胶合板／人工辅料","米",{"v":24,"d":"24.00"}]
[null,3,"安装造型不锈钢脚线","不锈钢／人工辅料","米",{"v":24,"d":"24.00"}]
[null,"十一","柜体/房间"]
[null,1,"M01房门","木饰面／含五金配件锁具","樘",{"v":6,"d":"6.00"}]
[null,2,"M04房门","木饰面／含五金配件锁具","樘",{"v":1,"d":"1.00"}]
[null,3,"休闲区/茶水间定制一体化柜","木饰面／石英石／岩板／不锈钢／人工辅料","m2",{"v":9.450000000000001,"d":"9.45"}]
[null,4,"开放式办公定制柜","木饰面／人工辅料","m2",3.24]
[null,5,"开放式办公定制层架","木饰面／人工辅料","m2",3.24]
[null,6,"会议室定制柜","木饰面／人工辅料","m2",3.54]
[null,7,"储物间／洽谈室／机房/打印室定制柜","木饰面／人工辅料","m2",3.54]
[null,8,"董事长办公室定制柜","木饰面／人工辅料","m2",3.54]
[null,9,"总经理办公室定制柜","木饰面／人工辅料","m",{"v":3.3,"d":"3.30"}]
[null,10,"副总经理办公室定制柜","木饰面／人工辅料","m",{"v":3.3,"d":"3.30"}]
[null,11,"财务办公室定制柜","木饰面／人工辅料","m",{"v":3.3,"d":"3.30"}]
[null,12,"男女更衣室定制柜","木饰面／人工辅料","m",{"v":3.3,"d":"3.30"}]
[null,null,"合计",{"$nulls":10},{"v":0,"d":"0.00"}]

{"sheet":"12F机电安装","index":5,"n_rows":123,"n_cols":15,"rows_kept":123,"merged":[[0,1,0,14],[1,1,1,9],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,2,13],[2,14,3,14]],"flags":["formulas_cached_only"]}
[null,"横琴南光大厦项目工程报价清单（机电安装）"]
[null,"工程名称：横琴南光大厦项目12F北大荒办公室精装修工程"]
[null,"序号","部位","项目名称","项目特征描述","计量单位","工程量","含税综合单价（元）","其中(元)",{"$nulls":5},"含税合价（元）\n"]
[{"$nulls":8},"人工","主材（含损耗）","机械费及辅材费等","管理费","利润","税金9%"]
[null,"一",null,"电气","","",""]
[null,"1",null,"配电箱","1、名称:配电箱27ALZ（改造，增加电表、开关）\n2、安装方式:嵌墙暗装\n3、其他参照相关施工图纸及说明","台","1.000"]
[null,"2",null,"配电箱","1、名称:配电箱27ALZ-2\n2、安装方式:嵌墙暗装\n3、其他参照相关施工图纸及说明","台","1.000"]
[null,"3",null,"配电箱","1、名称:配电箱 27ALEZ-1\n2、安装方式:嵌墙暗装\n3、其他参照相关施工图纸及说明","台","1.000"]
[null,"4",null,"镀锌桥架","1、名称:镀锌桥架\n2、规格:CT 200*100*1.2\n3、其他参照相关施工图纸及说明","m",60]
[null,"5",null,"桥架支架制作、安装","1、名称:桥架支架制作、安装\n2、材质:型钢\n3、其他参照相关施工图纸及说明","Kg",80]
[null,"6",null,"电力电缆 WDZB-YJY-4x25+1x16","1、名称:电力电缆\n2、型号规格:WDZB-YJY-4x25+1x16\n3、材质:铜芯\n4、其他参照相关施工图纸及说明","m","40.000"]
[null,"7",null,"电力电缆头","1、名称:户内热缩式铜芯电力电缆头\n2、规格:4*25+1*16\n3、材质、类型:铜芯，热缩式\n4、安装部位:户内\n5、电压等级:1kV以下\n6、其他参照相关施工图纸及说明","个","2.000"]
[null,"8",null,"铜芯线","1、名称:铜芯线\n2、型号规格:WDZB-BYJ-2.5\n3、材质:铜芯\n4、其他参照相关施工图纸及说明","m",3000]
[null,"9",null,"铜芯线","1、名称:铜芯线\n2、型号规格:WDZB-BYJ-4\n3、材质:铜芯\n4、其他参照相关施工图纸及说明","m",5000]
[null,"10",null,"温控器线 TT-k-30 0.6*1.0","1、名称:温控器线\n2、型号规格:TT-k-30 0.6*1.0\n3、材质:铜芯\n4、其他参照相关施工图纸及说明","m",120]
[null,"11",null,"配管","1、名称:电线管\n2、规格:SC20\n3、配置形式:明配\n4、其他参照相关施工图纸及说明","m",1800]
[null,"12",null,"配管","1、名称:电线管\n2、规格:JDG20\n3、配置形式:明配\n4、其他参照相关施工图纸及说明","m",160]
[null,"13",null,"温控开关（重新安装）","1、名称:温控开关（原拆除主材利旧）\n2、规格:230V 10A\n3、安装方式:暗装\n4、其他参照相关施工图纸及说明","个",10]
[null,"14",null,"单联单控暗开关","1、名称:单联单控暗开关\n2、规格:230V 10A\n3、安装方式:暗装\n4、其他参照相关施工图纸及说明","个","5.000"]
[null,"15",null,"双联单控暗开关","1、名称:双联翘板开关\n2、规格:230V 10A\n3、安装方式:暗装\n4、其他参照相关施工图纸及说明","个",20]
[null,"16",null,"三联单控暗开关","1、名称:三联翘板开关\n2、规格:230V 10A\n3、安装方式:暗装\n4、其他参照相关施工图纸及说明","个","2.000"]
[null,"17",null,"三联单控暗开关(重新安装)","1、名称:三联翘板开关（原拆除主材利旧）\n2、规格:230V 10A\n3、安装方式:暗装\n4、其他参照相关施工图纸及说明","个","9.000"]
[null,"18",null,"四联单控暗开关","1、名称:四联单控暗开关\n2、规格:230V 10A\n3、安装方式:暗装\n4、其他参照相关施工图纸及说明","个","1.000"]
[null,"19",null,"双联双控暗开关","1、名称:双联双控暗开关\n2、规格:230V 10A\n3、安装方式:暗装\n4、其他参照相关施工图纸及说明","个",4]
[null,"20",null,"普通单相五孔插座","1、名称:普通单相五孔插座\n2、规格:230V 10A\n3、安装方式:暗装\n4、其他参照相关施工图纸及说明","个",260]
[null,"21",null,"单相五孔地插","1、名称:单相五孔地插\n2、规格:230V 10A\n3、安装方式:暗装\n4、其他参照相关施工图纸及说明","个","7.000"]
[null,"22",null,"接线位","1、名称:接线位\n2、安装形式:暗装\n3、其他参照相关施工图纸及说明","个","23.000"]
[null,"23",null,"嵌入式办公灯盘 600*1200 ","1、名称:嵌入式办公灯盘 600*1200 \n2、产品参数：600*1200*35mm;功率:64W;色温:4000K \n3、其他参照相关施工图纸及说明","套",8]
[null,"24",null,"条形造型灯","1、名称:条形造型灯L2\n2、产品参数：功率:30W/m;色温:4000K \n3、其他参照相关施工图纸及说明","套",56]
[null,"25",null,"嵌入式调节射灯 L7","1、名称:嵌入式调节射灯 L7\n2、产品参数：φ86mm*H90mm;功率:12W;色温:4000K \n3、其他参照相关施工图纸及说明","套","16.000"]
[null,"26",null,"应急筒灯","1、名称:应急筒灯\n2、产品参数： \n3、其他参照相关施工图纸及说明","套","13.000"]
[null,"27",null,"消防应急标志灯具-单面左向","1、名称:消防应急标志灯具-单面左向\n2、规格：230V 5W\n3、其他参照相关施工图纸及说明","套",3]
[null,"28",null,"消防应急标志灯具-单面双向","1、名称:消防应急标志灯具-单面双向\n2、规格：230V 5W\n3、其他参照相关施工图纸及说明","套","2.000"]
[null,"29",null,"消防应急标志灯具-疏散出口","1、名称:消防应急标志灯具-疏散出口\n2、规格：230V 5W\n3、其他参照相关施工图纸及说明","套","9.000"]
[null,"30",null,"暗藏灯带","1、名称:暗藏灯带 \n2、尺寸：功率:12W;色温:4000K\n3、其他参照相关施工图纸及说明","m",60]
[null,"31",null,"开关插座盒","1、名称:开关插座盒\n2、安装形式:暗装\n3、其他参照相关施工图纸及说明","个",260]
[null,"32",null,"接线盒","1、名称:接线盒\n2、安装形式:暗装\n3、其他参照相关施工图纸及说明","个",180]
[null,"33",null,"凿槽及修补","1、名称:凿槽及修补\n2、规格:70mm×70mm\n3、类型:砖结构\n4、填充(恢复)方式:水泥砂浆修补","m",80]
[null,"二",null,"给排水","","",""]
[null,44,null,"PP-R给水管","1.名称：PP-R给水管\n2.规格：DN15\n3.连接方式：热熔连接\n4.管道消毒、冲洗","m",60]
[null,45,null,"角阀 DN15","1.名称：角阀\n2.规格：DN15","个",6]
[null,46,null,"洗涤盆","1.名称：洗涤盆\n2.含附件等全部工作内容","组","1.000"]
[null,47,null,"水龙头","1、不锈钢洗手盆水龙头\n2、其他参照相关施工图纸及说明","个",1]
[null,48,null,"UPVC排水管","1.名称：UPVC排水管\n2.规格：DN50\n3.连接方式：粘接连接","m",25]
[null,"三",null,"消防工程","",""]
[null,49,null,"闭式玻璃球喷头","1.名称：新增闭式玻璃球喷头(含上下喷）\n2.规格：T-ZSTZ 15-68℃\n3.其他：根据装修要求开孔、定位等完成本清单的一些工序","个",{"v":22,"d":"22.000"}]
[null,50,null,"闭式玻璃球喷头（重新安装）","1.名称：闭式玻璃球喷头（原拆除主材利旧）\n2.规格：T-ZSTZ 15-68℃\n3.其他：根据装修要求拆除、移位、开孔、定位等完成本清单的一些工序","个",{"v":60,"d":"60.000"}]
[null,51,null,"内外壁热镀锌钢管","1.名称：内外壁热镀锌钢管\n2.规格：DN50\n3.连接方式：螺纹连接","m",8]
[null,52,null,"内外壁热镀锌钢管","1.名称：内外壁热镀锌钢管\n2.规格：DN40\n3.连接方式：螺纹连接","m",9]
[null,53,null,"内外壁热镀锌钢管","1.名称：内外壁热镀锌钢管\n2.规格：DN32\n3.连接方式：螺纹连接","m",20]
[null,54,null,"内外壁热镀锌钢管","1.名称：内外壁热镀锌钢管\n2.规格：DN25\n3.连接方式：螺纹连接","m",80]
[null,55,null,"管道支架","1.名称：管道支吊架制作安装\n2.除锈刷油：防锈漆一道，调和漆一道","kg",3]
[null,56,null,"管道刷油","1.名称：管道刷油\n2.管道面漆一道","㎡",18]
[null,57,null,"自动报警系统调试","1、自动报警系统装置调试 64点以下\n2、其他参照相关施工图纸及说明","系统","1.000"]
[null,58,null,"感烟探测器（地址式）","1、名称:感烟探测器（新增）\n2、其他参照相关施工图纸及说明\n3、其他：根据装修要求开孔、定位等完成本清单的一些工序","个",6]
[null,59,null,"感烟探测器（地址式）重新安装","1、名称:感烟探测器（原拆除主材利旧）\n2、其他参照相关施工图纸及说明\n3、其他：根据装修要求开孔、定位等完成本清单的一些工序","个",20]
[null,60,null,"消防广播（重新安装）","1、名称:消防广播（原拆除主材利旧）\n2、其他参照相关施工图纸及说明\n3、其他：根据装修要求开孔、定位等完成本清单的一些工序","个",6]
[null,61,null,"报警线 WDZN-BYJF-2*1.5","1、名称:管内穿线\n2、型号规格:WDZN-BYJF-2*1.5\n3、材质:铜芯\n4、部位:室内\n5、其他参照相关施工图纸及说明","m",200]
[null,62,null,"广播线 WDZN-BYJF-2*1.5","1、名称:管内穿线\n2、型号规格:WDZN-BYJF-2*1.5\n3、材质:铜芯\n4、部位:室内\n5、其他参照相关施工图纸及说明","m",100]
[null,63,null,"配管 SC15","1、名称:镀锌钢管\n2、规格:SC15\n3、配置形式:明配\n4、其他参照相关施工图纸及说明","m",260]
[null,64,null,"金属软管  DN15","1、名称:金属软管\n2、规格:DN15\n3、配置形式:吊顶内敷设\n4、其他参照相关施工图纸及说明","m",30]
[null,65,null,"镀锌接线盒 86*86*50","1、接线盒 暗装\n2、镀锌接线盒 86*86*50","个",30]
[null,"四",null,"智能化系统","",""]
[null,66,null,"6芯单模光纤","1、名称:6芯千兆单模光纤\n2、型号规格:6芯\n3、敷设方式:线槽配线\n4、【工作内容】：敷设、测试\n5、其他参照相关施工图纸及说明","m",{"v":120,"d":"120.000"}]
[null,67,null,"100对大对数电缆","1、名称:室内大对数电缆\n2、型号规格:100对\n3、敷设方式:线槽配线\n4、【工作内容】：敷设、测试；卡接（配线架侧）\n5、其他参照相关施工图纸及说明","m",{"v":120,"d":"120.000"}]
[null,68,null,"弱电机柜 RX27A 18U","1、名称：标准机柜18U\n2、规格：防护等级：IP20；18U\n3、安装方式：落地式\n4、【工作内容】开箱检查、清洁搬运、安装固定、附件安装、接地等。\n5、其他按图纸及规范要求","台","1.000"]
[null,69,null,"24口交换机","1、名称： 24口接入交换机\n2、规格：L2+, 24 100/1000M RJ45接口+1个扩展卡插槽 \n3、【工作内容】安装、调试\n4、其他按图纸及规范要求","台",2]
[null,70,null,"16口POE交换机","1、名称： 16口接入交换机\n2、规格：L2+, 16 100/1000M RJ45接口（支持POE/POE+）+1个扩展卡插槽 \n3、【工作内容】安装、调试\n4、其他按图纸及规范要求","台","1.000"]
[null,71,null,"弱电机柜 RX27B 12U","1、名称：标准机柜12U1、名称：标准机柜12U\n2、规格：防护等级：IP20；12U\n3、安装方式：落地式\n4、【工作内容】开箱检查、清洁搬运、安装固定、附件安装、接地等。\n5、其他按图纸及规范要求","台","1.000"]
[null,72,null,"24口交换机","1、名称： 24口接入交换机\n2、规格：L2+, 24 100/1000M RJ45接口+1个扩展卡插槽 \n3、【工作内容】安装、调试\n4、其他按图纸及规范要求","台","2.000"]
[null,73,null,"8口POE交换机","1、名称： 8口接入交换机\n2、规格：L2+, 8 100/1000M RJ45接口（支持POE/POE+）+1个扩展卡插槽 \n3、【工作内容】安装、调试\n4、其他按图纸及规范要求","台","1.000"]
[null,74,null,"8口POE交换机","1、名称： 8口接入交换机\n2、规格：L2+, 8 100/1000M RJ45接口（支持POE/POE+）+1个扩展卡插槽 \n3、【工作内容】安装、调试\n4、其他按图纸及规范要求","台","1.000"]
[null,75,null,"16口POE交换机","1、名称： 16口接入交换机\n2、规格：L2+, 16 100/1000M RJ45接口（支持POE/POE+）+1个扩展卡插槽 \n3、【工作内容】安装、调试\n4、其他按图纸及规范要求","台","1.000"]
[null,76,null,"网络型硬盘录像机","1、名称:网络型硬盘录像机（监控）\n2、要求：含硬盘，30天录像存储时间\n3、其他参照相关施工图纸及说明","台","2.000"]
[null,77,null,"管理电脑","1、名称：管理工作站\n2、规格：I5处理器/内存4G/2G独显/硬盘1T/千兆网卡/鼠标键盘/LED21.5英寸\n3、【工作内容】设备开箱检验、就位安装、跳线制作、连接、软件安装、调试。\n4、其他按图纸及规范要求","台","2.000"]
[null,78,null,"室内无线AP","1、名称：POE无线AP（吸顶式）\n2、规格：室内双频吸顶无线接入点，采用内置天线，工作在802.11b/g/n/ac模式，双千兆上联，支持胖瘦模式切换，支持RAC及MACC管理，支持POE供电和本地供电（POE供电电源需单独采购\n3、其他参照相关施工图纸及说明","个",6]
[null,79,null,"室内彩色摄影机","【项目特征】\n1、名称：400W红外网络半球摄像机（POE)\n2、四百万像素1/3英寸CMOS图像传感器，低照度效果好，图像清晰度高可输出400万(2560×1440)@25fps支持H.265编码，压缩比高，超低码流最大红外监控距离30米\n【工作内容】\n1.本体安装；2.云台安装\n3.镜头安装；4.保护罩安装\n5.支架安装；6.调试\n7.试运行\n8、其他按图纸及规范要求","台","3.000"]
[null,80,null,"55寸LED电视一体机","1、名称：55寸LED电视一体机\n2、规格：55寸壁挂液晶一体机，可竖装。分辨率1920*1080。超薄款。亮度350cd/㎡。内含播放器，嵌入式 android操作系统，四核 CPU,1G 内存，8G固态硬盘。带终端播放软件\n3、【工作内容】安装、调试\n4、其他按图纸及规范要求","台",1]
[null,81,null,"80寸LED电视机一体机","1、名称：80寸LED电视一体机\n2、规格：80寸壁挂液晶一体机，可竖装。分辨率1920*1080。超薄款。亮度350cd/㎡。内含播放器，嵌入式 android操作系统，四核 CPU,1G 内存，8G固态硬盘。带终端播放软件\n3、【工作内容】安装、调试\n4、其他按图纸及规范要求","台",1]
[null,82,null,"电话+网络双孔插座","1、名称：双孔插座\n2、规格：数据+语音\n3、型号：阻燃性能UL94V-0级；带有防尘盖，带有标识条\n4、【工作内容】绑扎固定光纤、安装光纤连接器及面板、做标记等。\n5、其他按图纸及规范要求","个",60]
[null,83,null,"电话插座","1、名称:电话插座\n2、规格:带6类模块，面板\n3、安装方式:综合考虑\n4、其他参照相关施工图纸及说明","个","1.000"]
[null,84,null,"网络插座","1、名称:网络插座\n2、规格:阻燃性能UL94V-0级；带有防尘盖，带有标识条\n3、安装方式: 综合考虑\n4、其他参照相关施工图纸及说明","个",20]
[null,85,null,"门禁控制器","1、TCP/IP通讯方式  脱机工作 两种开门验证方式: 验证权限时限开门、刷卡直接开门。\n2、读头接口：2 组维根接口。提供5VDC 或12VDC 读头工作电源；\n3、输入：2组标准门状态输入，2组出门请示按钮输入，2组标准防撬状态输入； \n4、输出:2组门锁继电器输出，2组门报警电器输出盘/LED21.5英寸\n【工作内容】\n1、开箱检查、设备初验、安装设备、调整。\n2、其他按图纸及规范要求","台","2.000"]
[null,86,null,"门禁读卡器","1、名称：门禁读卡器\n2、读写距离：小于10CM； 通讯协议：Wiegand26通讯；\n3、 具有声光提示，可直观区分不同状态的卡片身份证和M1卡。\n【工作内容】\n1、开箱检查、设备初验、安装设备、调整、系统调试。\n2、其他按图纸及规范要求","台","2.000"]
[null,87,null,"电控锁","1、名称：电控锁\n2、规格：带门磁信号反馈带灯转换、280KG单门磁力锁。\n3、附件：磁力锁支架\n【工作内容】\n1、开箱检查、设备初验、安装设备、调整、系统调试。\n2、其他按图纸及规范要求","台","2.000"]
[null,88,null,"开门按钮","1、名称：开门按钮\n2、校线、挂锡、钻眼固定、安装、编码、调测。\n3、其他按图纸及规范要求\n4、其他参照相关施工图纸及说明","个","4.000"]
[null,89,null,"人脸识别","1、名称:人脸识别\n2、安装位置:门顶安装 \n3、要求：要求内部及外部人员出入管理是以使用者在人脸识别门禁设备上的数据比对作为基础，以计算机为后台处理工具，全面实现对通道控制区内出入人员的自动化管理。同时根据使用者登记记录能够快速自动生成用户所需的按时间等多种排序条件可导出的门禁记录报表等， 方便管理人员查询记录。同时亦是作为内部工作人员的自动考勤系统。\n4、其他参照相关施工图纸及说明","台","2.000"]
[null,90,null,"UTP6","1、名称:六类非屏蔽网络线\n2、型号规格:UTP CAT6\n3、敷设方式:管内配线\n4、【工作内容】：敷设、测试\n5、其他按图纸及规范要求","m",5000]
[null,91,null,"门禁电锁控制线 RVV-4*0.75","1、名称:门禁电锁控制线 RVV-4*0.75\n2、其他参照相关施工图纸及说明","m",50]
[null,92,null,"门禁按钮控制线 RVV-2*0.75","1、名称:门禁控制线 RVV-2*0.75\n2、其他参照相关施工图纸及说明","m",100]
[null,93,null,"配管","1、名称:电线管\n2、规格:PC20\n3、配置形式:明配\n4、其他参照相关施工图纸及说明","m",600]
[null,94,null,"镀锌桥架","1、名称:镀锌桥架\n2、规格:CT 200*100*1.2\n3、其他参照相关施工图纸及说明","m",80]
[null,95,null,"接线盒","1、名称:接线盒\n2、安装形式:暗装\n3、其他参照相关施工图纸及说明","个",150]
[null,96,null,"HDMI接口","1、名称:HDMI接口\n2、安装形式:\n3、其他参照相关施工图纸及说明","个",12]
[null,"五",null,"空调防排烟","",""]
[null,"",null,"空调风系统","",""]
[null,97,null,"镀锌钢板矩形风管 δ=0.5","1、名称:镀锌钢板通风管道\n2、形状:矩形\n3、规格:长边长≤320\n4、板材厚度:0.5mm\n5、接口形式:咬口\n6、其他：参照设计图纸及规范要求","m2",120]
[null,98,null,"空调风管保温","1、名称:空调风管保温\n2、材料:橡塑保温\n3、板材厚度:40mm\n5、其他：参照设计图纸及规范要求","㎡",120]
[null,99,null,"风管支架除锈、刷油","1、形式：吊托支架\n2、材质：碳钢(型钢综合)\n3、除锈、刷油：人工除锈、刷油\n4、其他：参照设计图纸及规范要求","kg",500]
[null,100,null,"空调百叶风口 800*120","1、名称:空调百叶风口\n2、规格:800*120\n3、其他:参照设计图纸及规范要求","个",6]
[null,101,null,"方形散流器 600*600","1、名称:方形散流器（原拆除主材利旧）\n2、规格:600*600\n3、其他:参照设计图纸及规范要求","个",38]
[null,102,null,"排烟防火系统","",""]
[null,103,null,"镀锌钢板矩形风管 δ=1.6","1、名称:镀锌钢板通风管道\n2、形状:矩形\n3、规格:长边长≤1000\n4、板材厚度:1.6mm\n5、接口形式:咬口\n6、其他：参照设计图纸及规范要求","m2",15]
[null,104,null,"排烟风管保温","1、名称:排烟风管保温\n2、材料:玻璃纤维\n3、板材厚度:35mm\n4、其他：用35mm厚的玻璃纤维做隔热层,钢丝网捆扎后,再抹15mm厚防火保温水泥做保护壳,让其耐火极限不低于1.0h，具体做法参照设计图纸及规范要求","㎡",15]
[null,105,null,"风管支架除锈、刷油","1、形式：吊托支架\n2、材质：碳钢(型钢综合)\n3、除锈、刷油：人工除锈、刷油\n4、其他：参照设计图纸及规范要求","kg",40]
[null,106,null,"280℃常闭电动排烟防火阀 500*320","1、名称:280℃电动排烟防火阀\n2、规格:500*320\n3、支架形式、材质:吊架、型钢综合\n4、支架除锈、刷油：人工除锈两遍、刷红丹两遍、刷色漆两遍\n5、其他:参照设计图纸及规范要求","个",6]
[null,107,null,"280℃常闭电动排烟防火阀 320*120","1、名称:280℃电动排烟防火阀\n2、规格:320*120\n3、支架形式、材质:吊架、型钢综合\n4、支架除锈、刷油：人工除锈两遍、刷红丹两遍、刷色漆两遍\n5、其他:参照设计图纸及规范要求","个","2.000"]
[null,108,null,"单层百叶排烟风口 1000*400","1、名称:单层百叶排烟风口\n2、规格:1000*400\n3、其他:参照设计图纸及规范要求","个","1.000"]
[null,109,null,"单层百叶排烟风口 800*400","1、名称:单层百叶排烟风口\n2、规格:800*400\n3、其他:参照设计图纸及规范要求","个","5.000"]
[null,110,null,"单层百叶排烟风口 800*350","1、名称:单层百叶排烟风口\n2、规格:800*350\n3、其他:参照设计图纸及规范要求","个","1.000"]
[null,111,null,"消防调试费",null,"项","1.000"]
[null,"六",null,"拆除部分","",""]
[null,112,null,"喷头拆除","1、名称:喷头拆除\n2、搬运至甲方指定地点、成品保护（保存二次利用）、清理现场\n3、其他参照相关施工图纸及说明","个",100]
[null,113,null,"感烟、感温探测器拆除","1、名称:感烟、感温探测器拆除\n2、搬运至甲方指定地点、成品保护（保存二次利用）、清理现场\n3、其他参照相关施工图纸及说明","个",20]
[null,114,null,"火灾报警扬声器拆除","1、名称:火灾报警扬声器拆除\n2、搬运至甲方指定地点、成品保护（保存二次利用）清理现场\n3、其他参照相关施工图纸及说明","个","9.000"]
[null,115,null,"拆除送回风口","1、名称:拆除送回风口\n2、搬运至甲方指定地点、成品保护（保存二次利用）、清理现场\n3、其他参照相关施工图纸及说明","个",60]
[null,116,null,"拆除面板灯 600*600","1、名称:拆除面板灯 600*600\n2、搬运至甲方指定地点、成品保护（保存二次利用）、清理现场\n3、其他参照相关施工图纸及说明","套",40]
[null,117,null,"拆除墙面插座","1、名称:拆除墙面插座\n2、搬运至甲方指定地点、成品保护（保存二次利用）、清理现场\n3、其他参照相关施工图纸及说明","套",38]
[null,118,null,"拆除温控开关","1、名称:拆除温控开关\n2、搬运至甲方指定地点、成品保护（保存二次利用）、清理现场\n3、其他参照相关施工图纸及说明","套",6]
[null,119,null,"拆除三联单控开关","1、名称:拆除三联单控开关\n2、搬运至甲方指定地点、成品保护（保存二次利用）、清理现场\n3、其他参照相关施工图纸及说明","套","9.000"]
[null,120,null,"拆除门禁系统（含刷卡器、按钮、门锁）","1、名称:拆除门禁系统（含刷卡器、按钮、门锁）\n2、搬运至甲方指定地点、成品保护（保存二次利用）、清理现场\n3、其他参照相关施工图纸及说明","套",2]
[null,121,null,"拆除玻璃门","1、名称:拆除玻璃门\n2、搬运至甲方指定地点、成品保护（保存二次利用）、清理现场\n3、其他参照相关施工图纸及说明","樘",2]
[null,"七",null,"合计",{"$nulls":10},{"v":0,"d":"0.00"}]

{"sheet":"总价措施费项目","index":6,"n_rows":19,"n_cols":6,"rows_kept":19,"merged":[[0,0,0,5],[1,0,1,5],[18,0,18,3]],"flags":["formulas_cached_only"]}
["横琴南光大厦项目精装修工程报价清单-措施项目费"]
["工程名称:横琴南光大厦项目12F北大荒办公室精装修工程"]
["序号","项目名称","数量","单位","金额\n(元)","备注"]
[null,"措施项目费","","","",""]
["1","安全文明措施费",{"v":1,"d":"1.00"},"项",null,""]
["2","脚手架搭拆措施费",{"v":1,"d":"1.00"},"项"]
[3,"公区及已完工程成品保护费",{"v":1,"d":"1.00"},"项"]
[4,"拆除及废料外运",{"v":1,"d":"1.00"},"项"]
[4.1,"架空地板掀起及复原（拆除的架空地板需保管妥当，需重新安装）",{"v":1,"d":"1.00"},"项"]
[5,"开荒保洁",{"v":1,"d":"1.00"},"项"]
[6,"消防报建报验及相关费用"]
[6.1,"消防设计及施工资质管理费",{"v":1,"d":"1.00"},"项"]
[6.2,"消防图纸设计（含修改）",{"v":1,"d":"1.00"},"项"]
[6.300000000000001,"消防图纸资料整理",{"v":1,"d":"1.00"},"项"]
[6.400000000000001,"消防图纸资料报送窗口",{"v":1,"d":"1.00"},"项"]
[6.500000000000002,"消防审验、安检、现场勘察",{"v":1,"d":"1.00"},"项"]
[6.600000000000002,"装修设计及施工资质管理、装修图纸设计（含修改）、装修图纸资料整理",{"v":1,"d":"1.00"},"项"]
[6.700000000000003,"消防设施第三方检测费",{"v":1,"d":"1.00"},"项"]
["合计",{"$nulls":3},{"v":0,"d":"0.00"},""]